

Technical Support and E-Warranty Certificate  [www.vevor.com/support](https://www.vevor.com/support" \t "_blank)

**Garage wall shelving**

**Model: HL2472**

We continue to be committed to provide you tools with competitive price.

"Save Half", "Half Price" or any other similar expressions used by us only represents an estimate of savings you might benefit from buying certain tools with us compared to the major top brands and doses not necessarily mean to cover all categories of tools offered by us. You are kindly reminded to verify carefully when you are placing an order with us if you are actually saving half in comparison with the top major brands.



**Garage wall shelving**

**MODEL:HL2472**

****

Have product questions? Need technical support? Please feel free to contact us:

**[CustomerService@vevor.com](mailto:CustomerService@vevor.com)**



**NEED HELP? CONTACT US!**

This is the original instruction, please read all manual instructions carefully beforeoperating. VEVOR reserves a clear interpretation of our user manual. The appearance of the product shall be subject to the product you received. Please forgive us that we won't inform you again if there are any technology or software updates on our product.

**SAFETY INSTRUCTIONS**

**WARNING:This product contains small parts. If swallowed, it will pose a choking hazard. Keep these small parts away from children !**

1. Before installation, take protective measures to avoid personal injury!


****

**EYE PROTECTION**  **FOOT PROTECTION DUST MASK PROTECTION WEAR**

1. The product must be installed on a wooden or concrete wall. Before installation, ensure that the bearing capacity of the wall does not exceed the maximum bearing capacity ! Please strengthen the structure of the wall in time to consolidate the bearing capacity of the wall ! Otherwise, the product may be damaged or personal injury may occur !
2. This product is for indoor use only. Outdoor use may cause product damage or personal injury.
3. Please check and confirm whether the screws are loose every two months.
4. At least two people to complete the installation.
5. Ensure that you have read the instructions and fully understood how to install. If you do not understand any of the installation steps, contact a professional installation personnel.

7. Do not overload ! Maximum capacity : 800 lbs **/**per layer**（evenly distributed）**

**Installation Preparation:**

****

**MODEL AND PARAMETERS**

|  |  |
| --- | --- |
| **Model** | **HL2472** |
| Number of Units | 2 |
| Shelving Surface Size | 72x24 inch |
| Maximum Bearing Capacity | 800 lbs /per layer（1600lbs in total） |
| Material | Steel |
| Color | Black |

**STRUCTURE DIAGRAM**

2

****

1


1.Brackets 2.Shelf

**COMPONENTS**

|  |  |  |  |
| --- | --- | --- | --- |
| **No.** | **Picture** | **Name** | **Qty** |
| 1 | 1678257224228 | Bracket | 8 |
| 2 | 1678257321976 | Shelf (Foldable) | 2 |
| 3 | 1677836049510 | L-shaped Wrench | 1 |
| 4 | 1678257631151 | Positioning Paper | 1 |
| 5 | **1677835434254** | Micro Level Vial | 1 |
| 6 | 1677835307555 | Expansion Plug-8\*58 | 24 |
| 7 | 1678071710167 | Washer-8.5 | 24 |
| 8 | 1677834985544 | Hexagon Self-tapping Screw-8\*60 | 24 |
| 9 | 1677834109907 | Cable Ties-12\*250 | 16 |
| 10 | 1678257471368 | User Manual | 1 |

**ASSEMBLY**

**STEP 1-A : Installation on Solid Concrete Walls**



P

3

2

1

6

5

4

3

2

1

Micro Level Vial


Positioning Paper

1. (The positioning paper should be reused 6 times.)Paste the positioning paper to the appropriate height, glue the Micro level vial to adjust the level, and then use the jackhammer to lightly drill out the anchor points.(See mark 1 above.)
2. Remove the positioning paper and repaste.(Note:Coincide with the hole outlined in Step 1.(See mark P above.)
3. Follow step 1,2 to gently drill out all anchor points.(See mark 1,2,3,4,5,6 above.)

Note:Make sure the four rows of holes are in the same horizontal line.

1. Remove the positioning paper and drill holes(Φ12x60mm) into the wall.



Expansion Plug-8\*58

****

1. After clearing the residual soil in the hole, tap the expansion plug into the hole completely.


Hexagon Self-tapping Screw-8\*60

Washer-8.5

1. Install the brackets. The screw must be screwed in completely !

**STEP 1-B : Installation on Wooden Wall Post**



P

3

2

1

Micro level vial

Positionin paper

6

5

4

3



2

1

1. (The positioning paper should be reused 6 times.)Paste the positioning paper to the appropriate height, glue the Micro level vial to adjust the level, and then use the jackhammer to lightly drill out the anchor points.(See mark 1 above.)
2. Remove the positioning paper and repaste.(Note:Coincide with the hole outlined in Step 1.(See mark P above.)
3. Follow step 1,2 to gently drill out all anchor points.(See mark 1,2,3,4,5,6 above.)

Note:Make sure the four rows of holes are in the same horizontal line.

1. Remove the positioning paper and drill holes(Φ5.5x60mm) into the wall.


 ****

Hexagon Self-tapping Screw-8\*60

Washer-8.5


1. Install the brackets. The screw must be screwed in completely and press tightly !

**STEP 2 : Installation of The Shelf**



The hinge is located at the bottom !

Locating Block

****

Use 2 cable ties to fix the grid and bracket.

The protruding length of both ends should be equally divided.

**MAINTENANCE**

1. Do not overload.
2. Please try to avoid putting wet items on shelves. Keep the warehouse not too wet.
3. Please check and confirm whether the screws are loose every two months.
4. Dust off regularly with a clean rag, and arrange items neatly on shelves.

**VEVOR STORE INC**

**9448 RINCHMOND PL #E RANCHO CUCAMONGA, California, 91730 United States of America**

****

**TechnicalSupport and E-Warranty Certificate**

**[www.vevor.com/support](https://www.vevor.com/support" \t "_blank)**